**ERKAT DRUM CUTTER Model-ER1500-3XQ**

**Specification & Features**

Service Weight 2,000 Kg

Nominal Power 120 kW

Rotation Speed 75 rpm

Optimum Oil Flow 205 l/min – 300 l/min

Max Torque @350 bar 23,400 Nm

Max Cutting force @350 bar 65,000N

Pick Shaft Diameter 30 mm

Number of Picks 44 pcs

Max Oil Flow @ 10 bar 320 l/min

Max Operating Pressure 350 bar

Suitable for material with uniaxial compressive strength upto 80 MPa

**Scope Of Supply:**

--Static Q Multibracket (with integrated water spray nozzles for dust suppression )

--Cutting head with standard picks with wear resistant, exchangeable wear sleeves

-- Spare motor cover plate incl. O-ring seal and screws

--Tool kit

--Operating manual and spare part list

--Hydraulic hoses ( Pressure line , return line & drain line) including pre-charge valve for return line

--Quick Coupler with Hyd Kit(Installation included)

-Installation of the unit at your site & Operator Training

--Installation of the unit on the machine at our workshop & Operator Training